{0}The printed picture is wider machine total length,printed canceled.@
{1}Horz adjust value has been changed during printing£¬update to config?@
{2}Vert adjust value has been changed during printing£¬update to config?@
{3}The wiper can not go back to home position@
{4}The Y direction length is over the limit@
{5}Click yes,the carriage will go to home position@
{6}The printed picture is wider machine total length,printed canceled.@
{7}Latest print is not finish, continue to print?@
{8}None paramater@
{9}Test finish.Horz adjust value %d, Diff color value %d, Vert step to musle %.4f,Update to config?@
{10}Error@
{11}Notice@
{12}Lifting motor abnormalities
@
{13}Doctor blade motor abnormalities
@
{14}The ink stack communication exception
@
{15}Lift the origin sensor is no response
@
{16}The origin of smears sensor is no response
@